David Bowyer, M1AEI has for some time now been preparing 12 volt winch systems for 40, 60, 80 and 100 ft Strumech Versatowers,
as well as similar other models like Radio Structures, Westower, Altron and Tennamast.
The prepared narrow drum TDS-12.0 waterproof winch systems come ready made up on galvanized back plates and spacers as required.
to ensure that the back plate does not interfere with the front tube.
The solenoids are repositioned with remote wiring to keep the weather off them (although they are sealed).
The rope fixing hole on the drum is prepared to get the original mast rope through twice.
We also disable the freespool (the yellow knob).
Finally, we fit an Anderson quick disconnect fitting on the end of the winch supply cables and another on a battery harness with battery posts on the other end, then bench test and run.
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